DONE:

1. Complete the verification of DLA\_LPE component.

2. Build the part of the testbench of whole DLA.

3. Transfer register model from based on register interface to based on HZZ interfce.

TO DO:

1. Complete the data transfer from ddr to weight buffer and to global buffer.